## CYD-Klipper

An implementation of a Klipper status display on an ESP32 + screen.
Uses Moonraker to fetch data.
Source code is available on GitHub.

### Changelog

### Donate

If you found this project helpful, please consider a donation to my Ko-Fi.
It would help out a lot in the development of this project, due to the need to buy the screens.
Thank you!

### Report Issues

If you experience any issues with this project, or have any feature requests for the project, please report them on the issues tab on Github.

### Install

Select your device from the list below and click 'Connect'.
Note: You may need to hold the 'BOOT' button on the device while pressing install.
The 2.8" Resistive and 3.5" Capacitive models are best suited (in my opinion) for CYD-Klipper.
Note for any resistive models: You can clear touch calibration by holding the BOOT button for 8 seconds while the screen is on.